**University of Engineering and Technology, Peshawar**

Department of Computer Systems Engineering.

*Course : CSE-303 Microprocessor Based System Design*



**Zainab Khalid 19** PWCSE **1743**

Section A

Batch 21 (Spring\_2022)

**Submitted to** Dr, Bilal Habib

**TASK 5:**

**TASK 5:**

At a Motorway entry point in Peshawar, assume there are only two lanes to enter. One is for small vehicles and another one is for large ones. We have connected a sensor at each entry point. The sensor sends a signal (high-to-low edge) to our embedded system whenever a vehicle passes through the entry point and enters the Motorway. Use an 89C51 to count the number of vehicles passed through the entry point in one minute. As soon the one-minute time is over, it is indicated by turning ON a led at P3.1 pin, send the final value of small vehicles to Port-1 and larger ones to Port-2. Finally, the program goes into an infinite loop, doing nothing.

***• Draw schematic along with timing diagram. The oscillator frequency is 12MHz.***

***• Entry of a vehicle can be simulated using a button press.***

***• Use two buttons: one for large vehicles and another one for smaller ones.***

***• Use port interrupts at P3.2 and P3.3.***

***• Use seven segments to display count of vehicles at Port 1 and Port 2.***

***• Use timers for creating a delay of 1 min.***

Hint: Use timer interrupt and port interrupt. Use C language and Proteus ONLY.

**CODE:**

#include<reg51.h>

#include<stdio.h>

sbit s\_vehicle =P3^2;

sbit l\_vehicle=P3^3;

sbit led=P3^1;

int x=0;

int count1=0;

int count2=0;

void start\_timer1()

{

TR1=1;

}

void interpt\_1()interrupt 0

{

count1=count1+1;

}

void interpt\_2()interrupt 2

{

count2=count2+1;

}

void timer1() interrupt 3

{

x++;

if(x==1000)

{

led=1;

P1=count1;

P2=count2;

while(1)

{

}

}

TH1=0x15;

TL1=0x9F;

}

void init\_timer1()

{

TMOD=0x10;

TH1=0x15;

TL1=0x9F;

IE=0x8D; //external 0 interrpt and timer interrpt

IT0=1; //edge triggering

IT1=1;

s\_vehicle=1;

l\_vehicle=1;

}

void main()

{

led=0;

P1=0;

P2=0;

init\_timer1();

start\_timer1();

while(1)

{

}

}

**OUTPUT:**

